Lime

3.Quality inspection entering the warehouse. Warehouse.

Entering the warehouse

**Product packing**

2

Acceptable product

Product bin

Compactor

dryer

Primary separation

CL2+NAOH

Primary reaction

2

Buffer tank

1. Quality inspection of raw materials.

2. Quality inspection four place for the whole production line every two hours.

2

2

Large particles

Fines

Primary filter cake

Primary mother liquid

Lime bin

Product screen

Granulator

Product surge bin

Mixer